
L3HARRIS 787 Briefing Station

Quick Start Guide

***\*\* Start This Guide at the section relevant to condition the Briefing Station is found in \*\****

1. Turn on briefing station computer *(Figure 1)*
2. “Splash” the launch program will auto start *(Figure 2)*. If Splash is not running, click the icon on task bar to open Splash *(Figure 3)*

Splash program and Start Instance



Launch Splash Icon

1. Select correct Load (latest date) and Fit (VHZNP\_BRF)
2. Click on the “Start Instance button” *(Figure 2)*
3. Briefing program will load. Progress can be seen under “Console” **Note**: This may take a few minutes.
4. Flight Deck and the IOS panels will display
5. IOS and Flight Deck can be navigated using the Mouse and the Screens are also “*touch* *screens”*
6. Access the user guide by either pressing **F1** on keyboard or selecting the **Help** menu then **Contents** the user guide will open in an IE window**.**

Click on **Allow Blocked Content**

As a minimum read the **Hints and Tips** section

1. The Aircraft will be in a “de powered” state
2. Power up the Aircraft as per below
   * Set park Brake
   * Sim Freeze off
   * Battery Switch On
   * Wait 15 seconds after Capt Inboard and Lower EICAS screens display before proceeding
   * Select External Power on IOS and Overhead Panel or Start APU
3. Operate as per Simulator with the addition that if positioned on threshold aircraft will “auto takeoff” when a TOGA button is pressed. Engage an A/P airborne. Above 200’ before 2000’.

**\*\* When finished using the Briefing Station please leave the Station as you would leave the FF Simulator\*\***